Ravenbrook / Projects / Memory Pool System / Version 1.111 Product Sources / Design Documents

Memory Pool System Project

          DESIGN OF THE MANUALLY-MANAGED VARIABLE-SIZE FIRST-FIT POOL
                              design.mps.poolmvff
                                 incomplete doc
                               gavinm 1998-09-09

    INTRODUCTION

    .intro: The pool was created in a response to a belief that EPDL/EPDR's first
    fit policy is beneficial for some classes of client behaviour, but the
    performance of a linear free list was unacceptable.  This pool implements a
    first (or last) fit policy for variable-sized manually-managed objects, with
    control over first/last, segment preference high/low, and slot fit low/high.

    Document History

    .hist.0: GavinM wrote a list of methods and function plus some notes 1998-09-09.

    .hist.1: Added overview, removed bogus ArenaEnter design, and described
    buffered allocation.  pekka 1999-01-06

    .hist.2: Modified for the "Sunset On Segments" redesign of segments. Buffered
    allocation is no longer limited to segment boundaries.

    OVERVIEW

    .over: This pool implements certain variants of the address-ordered first-fit
    policy.  The implementation allows allocation across segment boundaries.
    .over.buffer: Buffered allocation is also supported, but in that case, the
    buffer-filling policy is worst-fit.  Buffered and unbuffered allocation can be
    used at the same time, but in that case, the first ap must be created before
    any allocations. .over.buffer.class: The pool uses the simplest buffer class,
    BufferClass. This is appropriate since these buffers don't attach to segments,
    and hence don't constrain buffered regions to lie within segment boundaries.
    .over.segments: The pool uses the simplest segment class (SegClass). There's no
    need for anything more complex.

    METHODS

    .method: The MVFF pool supports the following methods:

    .method.init: Res MVFFInit(Pool pool, va_list arg)
      This takes six vararg parameters:
      - extendBy -- the segment size;
      - avgSize -- the average object size;
      - alignment -- the alignment of allocations and frees (must be at least
    sizeof(void*));
      - slotHigh -- whether to allocate objects at the end of free blocks found, as
    opposed to at the start (for unbuffered allocation);
      - arenaHigh -- whether to express SegPrefHIGH to the arena, as opposed to
    SegPrefLOW;
      - firstFit -- whether to use the suitable block of lowest address, as opposed
    to the highest (for unbuffered allocation).
    .method.init.epdl: To simulate the EPDL pool, specify extendBy, avgSize, and
    maxSize as normal, and use slotHigh=FALSE, arenaHigh=FALSE, firstFit=TRUE.
    .method.init.epdr: To simulate the EPDL pool, specify extendBy, avgSize, and
    maxSize as normal, and use slotHigh=TRUE, arenaHigh=TRUE, firstFit=TRUE.
    .method.init.other: The performance characteristics of other combinations are
    unknown.

    .method.finish: The PoolFinish method,

    .method.alloc: Alloc and Free methods are supported, implementing the policy
    set by the pool params (see .method.init).

    .method.describe: The usual describe method.

    .method.buffer: The buffer methods implement a worst-fit fill strategy.

    EXTERNAL FUNCTIONS

    .function: MVFF supports the following external functions:

    .function.free-size: size_t mps_mvff_free_size(mps_pool_t pool)
      This function returns the total size of free space in segments allocated to
    the MVFF pool instance.

    .function.size: size_t mps_mvff_size(mps_pool_t pool)
      This function returns the total memory used by pool segments, whether free or
    allocated.

    .function.class: mps_class_t mps_class_mvff(void)
      This function returns the class object for the pool class, to be used in pool
    creation.

    IMPLEMENTATION

    .impl.free-list: The pool stores its free list in a CBS (see design.mps.cbs).
    It uses the CBS's mayUseInline facility to avoid running out of memory to store
    the free this.  This is the reason for the alignment restriction above.

    DETAILS

    .design.seg-size: When adding a segment, we use extendBy as the segment size
    unless the object won't fit, in which case we use the object size (in both
    cases we align up).

    .design.seg-fail: If allocating a segment fails, we try again with a segment
    size just large enough for the object we're allocating.  This is in response to
    request.mps.170186.

## A. References

## B. Document History

2002-06-07 | RB | Converted from MMInfo database design document.

## C. Copyright and License

This document is copyright © 1995-2002 Ravenbrook Limited. All rights reserved. This is an open source license. Contact Ravenbrook for commercial licensing options.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met:

1. Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer.
2. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution.
3. Redistributions in any form must be accompanied by information on how to obtain complete source code for the this software and any accompanying software that uses this software. The source code must either be included in the distribution or be available for no more than the cost of distribution plus a nominal fee, and must be freely redistributable under reasonable conditions. For an executable file, complete source code means the source code for all modules it contains. It does not include source code for modules or files that typically accompany the major components of the operating system on which the executable file runs.

This software is provided by the copyright holders and contributors "as is" and any express or implied warranties, including, but not limited to, the implied warranties of merchantability, fitness for a particular purpose, or non-infringement, are disclaimed. In no event shall the copyright holders and contributors be liable for any direct, indirect, incidental, special, exemplary, or consequential damages (including, but not limited to, procurement of substitute goods or services; loss of use, data, or profits; or business interruption) however caused and on any theory of liability, whether in contract, strict liability, or tort (including negligence or otherwise) arising in any way out of the use of this software, even if advised of the possibility of such damage.

`$Id: //info.ravenbrook.com/project/mps/version/1.111/design/poolmvff/index.html#2 $`

Ravenbrook / Projects / Memory Pool System / Version 1.111 Product Sources / Design Documents